MuonGeoModel deliv.

no test yet of simulation reading cond. data

need to re-tag the test folder in COOL with alignment data

We should define clearly the strategy (Geometry tags and Condition tags) for our non official exercise of simulation + reconstruction with condition data

resume clash survey

in cooperation with Alexander K.

Laurent C. recently spot a small clash to be investigated

cutouts

Optimization of RE

MDT class in place – submitted for 14.0.0

Other technologies to come (can they go in 14.0.x or should we move to 14.x.0 ?)

B-lines access to cond. DB and validation (against Amdc)

needs the format of the Bline class to follow up the new convention (Andrea F.? when can we do that ?)

Andrei Barashkou provided a test description of the Saddle with BREPS for MuonGeoModel

Person power (on the MuonGeoModel active material + reco interfaces) is 0.3 %, i.e. LOW !

1 FTE would be desirable – this still leaves out the topics typically covered by Laurent which are heavier !!!

2008-02-07T11:01:11